08/26/2024

211-fp14.docx

|  |
| --- |
| Use on all projects with roadway obliteration. |

## Section 211. — ROADWAY OBLITERATION

**Description**

**211.01 (a) Method 1.** Add the following:

Blend obliteration areas into the adjacent natural ground along the horizontal and vertical planes by gradually transitioning obliteration slopes to remove noticeable breaks.

**Construction Requirements**

**211.02.** Delete this Subsection and substitute the following:

**211.02 Material Handling.**

**(a) Rigid material.** Remove rigid material according to Section 203. Dispose of material according to Federal, state, and local rules and regulations.

**(b) Nonrigid material.**

**(1) Nonasphalt material.** Scarify or rip the gravel, crushed stone, or other nonrigid surface, base, and subbase material. Mix the scarified or ripped material with the underlying soil. Bury the mixture under at least 12 inches (600 millimeters) of onsite soil.

**(2) Asphalt contaminated material.** Dispose of asphalt contaminated material according to Subsection 203.05.

**Measurement**

**211.05** Add the following:

Do not measure areas within slope stake limits under roadway obliteration.

Measure material excavated from an obliterated roadway and used for new construction or in separate obliteration locations under Section 204.