|  |
| --- |
| Use with gabions or revet mattresses, as applicable. |

## Section 253. - GABIONS AND REVET MATTRESSES

**Material**

**253.02** Add the following**:**

Select granular backfill 704.08

**Construction Requirements**

|  |
| --- |
| Include 253.03 with all projects that have gabions walls |

**253.03 General.**  Delete the first sentence and substitute the following:

Survey according to Section 152 and verify the limits of the structure.

|  |
| --- |
| Include 253.05 with all projects that have gabions walls |

**253.05 Structure Erection.** Add the following to the first paragraph:

For gabion structures, grade the foundation for a width equal to the width of the gabion plus 2 feet (0.6 meters). Where gabions are set on rocky foundations, place 6 inches (150 mm) of select granular backfill under the baskets.