02/25/2025

Include if project has structural concrete removal. Verify with Bridge. Edit hammer impact strength if necessary to meet project-specific conditions.

## Section 572. — CONCRETE REPAIR

**572.06. Concrete Repair.** Delete the second sentence of the first paragraph and substitute the following:

Use power-driven hand tools and other hand tools to remove existing concrete. Do not use jackhammers heavier than 30 pounds. Do not operate jackhammers and mechanical chipping tools at an angle more than 45 degrees measured from the surface of the concrete.