04/21/2025

## Section 602. — CULVERTS AND DRAINS

Include if project has heat fusion welding HPDE pipe for lining culverts or when constructing long rundowns.

**Construction Requirements**

**602.03 General**. Add the following:

Provide heat fusion welded HDPE pipe with a rating of DR 21, 100 psi or higher. Heat fuse pipe according to ASTM F2620.