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Include if using rolled erosion control products or cellular confinement systems.
Section 629. — ROLLED EROSION CONTROL PRODUCTS AND CELLULAR CONFINEMENT SYSTEMS
629.06(a)(3) Check slot. Delete this Subsection and substitute the following:
[bookmark: _Hlk132013183](3) Check slot. Install two rows of fasteners 4 inches apart on 4-inch centers across the top edge of the RECP. Drive fasteners flush with soil surface.

629.06(b) Channel installations. Delete the second paragraph and substitute the following:
Securely fasten RECP to the soil by installing fasteners at a minimum rate of 2 per square yard. Significantly higher anchor rates may be necessary in sandy, loose, or wet soils and in severe applications. 
629.07 Cellular Confinement Systems. Delete the first paragraph and substitute the following:
Excavate to the depth of the cellular confinement system and smooth and compact the slope. Install the top of the system flush or lower than the adjacent slope. Expand the geocell down the slope. Connect adjacent geocell sections with fasteners in every other cell.
