*INCLUDE SECTION 104 ON ALL PROJECTS WITH CLAUSE $$104.06A AS A MINIMUM*

$$104.00A

Section 104. — CONTROL OF WORK

Revised 24 May 2024

*INCLUDE THE FOLLOWING ON ALL PROJECTS*

$$104.06A

104.06(c). Add the following to the first paragraph:

Provide one full-size (22- by 34-inch) paper copy of the plans from the Government-furnished electronic plans and use this set of plans exclusively for as-built drawings.

*INCLUDE THE FOLLOWING ON NPS PROJECTS (IF INCLUDING FOR OTHER PARTNERS, MAKE APPROPRIATE EDITS)*

$$104.08A

104.08. Add the following to the second paragraph:

When hauling on National Park Service roads, do not exceed the load restrictions shown in Table 104-1.

|  |  |
| --- | --- |
| **Table 104-1**  **Load Restrictions** | |
| **Single Units** | **Gross Vehicle Weight, pounds** |
| 2 axles | 40,000 |
| 3 axles | 48,000 |
| 4 or more axles | 52,000 |
| **Combination Units** | **Gross Vehicle Weight, pounds** |
| 3 axles | 57,000 |
| 4 axles | 62,000 |
| 5 or more axles | 66,000 |

Where the ground is saturated with water or during periods of freezing and thawing, the CO may impose further load restrictions or suspend hauling.

*INCLUDE THE FOLLOWING SPEC INSTRUCTION LINE IF ANY OF THE CLAUSES $$104.08C, $$104.08D, OR $$104.08E ARE INCLUDED*

$$104.08B

104.08. Add the following:

*INCLUDE THE FOLLOWING IF HAULING MATERIALS INTO THE PROJECT (VERIFY WITH THE PARTNER AND DISCUSS WITH CONSTRUCTION)*

$$104.08C

Hauling will only be permitted from the nearest point of public access to the work site. Minimize hauling over completed pavement.

*INCLUDE THE FOLLOWING IF RESTRICTING ACCESS TO THE PROJECT THROUGH A SPECIFIC ROADWAY (VERIFY WITH THE PARTNER AND DISCUSS WITH CONSTRUCTION)*

$$104.08D

Do not use *(insert roadway name)* to access the project site during construction.

*INCLUDE THE FOLLOWING IF HAULING MATERIALS INTO THE PROJECT (VERIFY WITH THE PARTNER AND DISCUSS WITH CONSTRUCTION)*

$$104.08E

Operate loaded vehicles hauling material at speeds not exceeding 40 miles per hour or the posted speed limit, whichever is lower, and spaced at 500-foot minimum intervals. When hauling on bridges, do not exceed 25 miles per hour or the posted speed limit, whichever is lower, or operate more than 1 loaded hauling vehicle at a time.

*INCLUDE THE FOLLOWING IF THERE IS THE POSSIBILITY OF OTHER CONSTRUCTION PROJECTS OCCURRING IN THE VICINITY*

$$104.11A

104.11. Add the following:

Coincident with this contract, other contracts for construction projects may be underway or may commence during the construction of this project. Coordinate with the CO and other contractors to minimize disruption to this project and to other construction projects in the area.