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INCLUDE CLAUSE $$721.01A WHEN INSTALLING PULL BOXES FOR TRAFFIC COUNTERS (IF USED, ALSO INCLUDE APPLICABLE SECTION 636 CLAUSES)
$$721.01A
721.01(b).  Add the following:

Provide boxes fabricated with fiberglass reinforced polymer concrete conforming to ANSI/SCTE 77 and tier 22 loading.

Provide a waterproof, detachable, cast iron lid conforming to AASHTO M 105, Class 30 with lift opening.  Ensure the pull slots are rated for a minimum pull out of 3,000 pounds and the pull boxes are rated for a minimum wheel load of 20,000 pounds.  Provide stainless steel lock down bolts for the lid.

INCLUDE CLAUSE $$721.01B FOR NEW CONSTRUCTION OR FULL DEPTH PAVEMENT PROJECTS
$$721.01B
As an acceptable alternative to sawcutting, provide preformed inductive loops with 3 to 5 turns of #14 AWG cable with an insulation of XLPE (cross-linked polyethylene) encased in PVC pipe for use in new construction before the pavement is installed.

INCLUDE CLAUSE $$721.01C FOR BONDING EQUIPMENT AND HARDWARE WHEN MOUNTING CABINET ON A POLE
$$721.01C
721.01(f).  Add the following:

Provide high strength, corrosion resistant mounting bracket, pole clamps, and related hardware.

Provide galvanized anchor bolts, nuts, lock washers, and flat washers conforming to ASTM A153.

INCLUDE CLAUSE $$721.01D FOR SPLICES AND CRIMPS
$$721.01D
721.01(l).  Add the following:

Provide industrial grade copper-alloy wire crimps of appropriate size.  Do not splice with wire nuts.  Comply with MIL-T-7928.  Do not use vinyl plastic electrical tape or liquid electrical coating as a splicing material.  If needed for insulation protection, provide cold and weather resistant, ¾-inch wide, ¼-inch thick tape and a compatible fast drying sealant applied by brush.

If soldering splice, provide electronic-grade, rosin-core, 60 lead/40 tin solder.  Do not use acid-core solder or acid-type soldering pastes.

INCLUDE CLAUSE $$721.02A FOR POLE AND CABINET PAINT REQUIREMENTS.  INCLUDE THE CLAUSE WHEN A NEW CABINET IS INSTALLED, REGARDLESS OF IT BEING MOUNTED ON A POLE OR NOT (IF USED, VERIFY WITH PARTNER AGENCY IF THE COLOR CODE IS CORRECT AND REVISE AS NECESSARY)
$$721.02A
721.02(a).  Delete the second sentence of the last paragraph and substitute the following:

For the finished coat for the pole and inside and outside of the cabinet, use epoxy modified enamel matching Federal Standard 595B Color No. 20059 (brown), unless otherwise approved. 





