## Section 251. — RIPRAP

01 APR 2024 – FP-24

Construction Requirements

WFL Specification 01 APR 2024 2510010

Include the following when there is limited vertical clearance to work (i.e. under bridges, in box culverts).

Edit as required for non-bridge work.

### 251.03 General.

Add the following:

Place riprap under or adjacent to structures before placing prefabricated superstructure units or constructing superstructure falsework.