## Section 636. — TRAFFIC SIGNAL, TRAFFIC COUNTER, LIGHTING, AND ELECTRICAL SYSTEMS

01 APR 2024 – FP-24

Measurement

WFL Specification 01 APR 2024 6360010

Include the following when:

1. the project includes pay items for both conduits and utility trenches, and;
2. the conduits in the utility trenches are incidental to the utility trench pay item, and;
3. the pay items are not lump sum

Edit description and location as needed.

### 636.13

Add the following:

Do not measure conduits installed in the following utility trenches:

**Description**  **Location**

[INSERT TRENCH PAY ITEM NAME] [INSERT STA/OFFSET LOC.]

[INSERT TRENCH PAY ITEM NAME] [INSERT STA/OFFSET LOC.]

[INSERT TRENCH PAY ITEM NAME] [INSERT STA/OFFSET LOC.]

WFL Specification 01 APR 2024 6360020

Include the following when:

1. the project includes pay items for conduits, and;
2. each conduits run in the utility trench is intended to be paid for, regardless of whether it is a single conduit in a trench or multiple conduits in a single trench, and;
3. the pay items are not lump sum.

### 636.13

Add the following:

Measure conduits by the linear foot, including each conduit run placed in a singular trench.