08/26/2024

261-fp14.docx

|  |
| --- |
| Use on all projects with reinforced soil slopes. (Verify actual pay items with geotech – CFL doesn’t use square foot face pay item for RSS). |

## Section 261. — REINFORCED SOIL SLOPES

**Construction Requirements**

**261.04 General.** Delete the second paragraph and substitute the following:

Survey according to Section 152 and verify the limits of the reinforced soil slope installation.

Add the following:

Install underdrain system according to Section 605 if shown in the plans.

**Measurement**

**261.07** Delete the second paragraph and add the following:

Measure earthwork under Section 204.

Measure reinforcement under Section 207.