08/26/2024

555-fp14.docx

|  |
| --- |
| When steel structures are required include Section 562 and the following: |

## Section 555. — STEEL STRUCTURES

**Construction Requirements**

|  |
| --- |
| The AISC Quality Certification Program identifies categories related to bridge fabrication. Insert the applicable category. Coordinate with the Bridge Engineer. |

**555.07 Fabrication.** Delete the first sentence of the first paragraph and substitute the following:

Fabricate the structural steel in a fabricating plant that is Certified Bridge Fabricator-Simple (SBR), Certified Bridge Fabricator-Intermediate (IBR) OR Certified Bridge Fabricator-Advanced (ABR) with supplemental program requirements for: Applicators of Complex Coatings Endorsement (CCE) or Fracture Control Endorsement (FCE), under the AISC, *Quality Certification Program*.

|  |
| --- |
| The AISC Quality Certification Program identifies categories related to bridge erection. Insert the applicable category. Coordinate with the Bridge Engineer. |

**555.18 Erection.** Delete the text of the second sentence of the first paragraph and substitute the following:

Use steel erector certified under the Certification Program for Erectors (CSE) with Seismic Endorsement, Metal Deck Endorsement, or Bridge Endorsement under the AISC, *Quality Certification Program*.