11/05/2015

S569-14\_11052015.docx

|  |
| --- |
| Use on projects when a concrete overlay for a bridge deck is required. |

## Section 569. — CONCRETE OVERLAYS FOR BRIDGE DECKS

**Construction Requirements**

**569.04 Composition (Concrete Mix Design).** Delete the first two paragraphs and substitute the following:

Design and produce concrete mixtures that conform to Table 569-1 for the class specified.

Submit concrete overlay mix designs on FHWA Form 1608, *552 Structural Concrete Mix Design Submittal* and determine the required average concrete compressive strength (fcr) with $\overbar{X}$ ≥ fcr.

Delete the first sentence of the third paragraph and substitute the following:

Verify mixture design with trial mixes from proposed sources or with previous concrete production data for the mixture design submitted from proposed sources.