05/12/2015

S603-14\_05122015.docx

|  |
| --- |
| Use the following with projects requiring structural steel plate structures:. |

## Section 603. — STRUCTURAL PLATE STRUCTURES

**603.04** **Erecting.** Delete the seventh paragraph and substitute the following:

Torque steel bolts and aluminum bolts on 0.1-inch (205-millimeter) thick and heavier aluminum plates to at least 115 foot-pounds (155 newton-meters) and a maximum of 130 foot-pounds (180 newton-meters).