## Section 104. — CONTROL OF WORK

01 JUL 2024 – FP-24

WFL Specification 01 APR 2024 1040010

Include the following in projects containing concrete box culverts when load ratings are not required.

Coordinate with WFL Structures to determine the need for load ratings.

### 104.06 Specifications and Drawings.

Delete Subsection (b)(2)*(k)* and substitute the following:

*(k)* Concrete box culvert and precast or cast-in-place concrete foundations details;

WFL Specification 01 APR 2024 1040020

Include the following in projects containing concrete box culverts when load ratings are required.

Coordinate with WFL Structures to determine the need for load ratings.

### 104.06 Specifications and Drawings.

Delete Subsection (b)(2)*(k)* and substitute the following:

*(k)* Concrete box culvert with load ratings and supporting calculations, and precast or cast-in-place concrete foundations details;

WFL Specification 01 APR 2024 1040030

Include the following in MATOC projects.

### 104.07 Coordination of Contract Documents.

Delete the text of this Subsection and substitute the following:

The FAR, TAR, Basic Contract, Special Contract Requirements (SCR), plans, and Standard Specifications are contract documents. A requirement in one document is binding as though occurring in all the contract documents. The contract documents are intended to be complementary and to describe and provide for a complete contract. In case of discrepancy, calculated and shown dimensions govern over scaled dimensions. The contract documents govern in the following order:

**(a)** FAR;

**(b)** TAR;

**(c)** Basic IDIQ Contract;

**(d)** SCR;

**(e)** Plans; and

**(f)** Standard Specifications.

WFL Specification 01JUL 2024 1040040

Include the following with:

1. NPS projects, and;

2. When the *FLH Bridge Oversized/Overweight Permit Load Request* form is provided as physical data

### 104.08 Load Restrictions.

Add the following:

Submit oversized and overweight permit requests for non-legal loads transported within the [INSERT PARK NAME] National Park boundary. Use the *FLH Bridge Oversized/Overweight Permit Load Reques*t form listed under FAR Clause 52.236-4 Physical Data (Apr 1984).

WFL Specification 01 APR 2024 1040050

Include the following when other contracts in close proximity may have an effect on this project. List point of contact if applicable.

### 104.11 Other Contracts.

Add the following:

[INSERT LANGUAGE].