## Section 708. — PLASTIC PIPE

01 APR 2024 – FP-24

WFL Specification 01 APR 2024 7080010

Include the following when underdrain pipe less than or equal to 10 inches is required.

### 708.04 Corrugated polyethylene drainage tubing.

Delete this subsection and substitute the following:

Furnish perforated and nonperforated 3- to 10‑inch diameter tubing conforming to AASHTO M 252, Type C or CP.